#
DTC TABLE

id0802a0800600

• DTCs are common to present and past malfunction diagnosis.

  Note

  • When DTCs not shown in the DTC table are displayed, replace the SAS control module.
  • If the air bag system warning light does not illuminate or remains illuminated when the ignition switch is turned to the ON position, inspect and repair the air bag system warning light circuit, and then confirm that the air bag system warning light is operational.
  • The air bag system warning light flashes the DTC pattern for five cycles, and then remains illuminated until the ignition switch is turned to the LOCK position.
  • If the SAS control module configuration is performed while the air bag system circuit has a malfunction, the air bag system warning light flashes. Verify that the warning light goes off approx. 15 s after the system circuit malfunction is solved.

DTC | Malfunction location | Page
--- | --- | ---
WDS display | Air bag system warning light
B1231 | 13 |  | SAS control module activation (deployment) control freeze | (See DTC B1231.)
B1317 | - | Continuously illuminated | The power supply voltage increases (16.1 V or more). | (See DTC B1317, B1318.)
B1318 | - | Continuously illuminated | The power supply voltage decreases (less than 9 V).
B1342 | 12 |  | SAS control module | (See DTC B1342.)
- | Continuously illuminated | SAS control module (DTC 12 detection circuit malfunction)
B1869 | - | Continuously illuminated | Air bag system warning light system circuit open | (See DTC B1869, B1870.)
- | Does not illuminate | Air bag system warning light system circuit short to ground
B1870 | - | Continuously illuminated | Air bag system warning light system circuit short to power supply
B1877 | 33 |  | Driver-side pre-tensioner seat belt system circuit resistance high | (See DTC B1877, B1878, B1879, B1885.)
B1878 | Driver-side pre-tensioner seat belt system circuit short to power supply
B1879 | Driver-side pre-tensioner seat belt system circuit short to ground
B1881 | 34 |  | Passenger-side pre-tensioner seat belt system circuit resistance high | (See DTC B1881, B1882, B1883, B1886.)
B1882 | Passenger-side pre-tensioner seat belt system circuit short to power supply | (See DTC B1881, B1882, B1883, B1886.)
B1883 | Passenger-side pre-tensioner seat belt system circuit short to ground | (See DTC B1881, B1882, B1883, B1886.)
B1885 | 33 |  | Driver-side pre-tensioner seat belt system circuit resistance low | (See DTC B1877, B1878, B1879, B1885.)
B1886 | 34 |  | Passenger-side pre-tensioner seat belt system circuit resistance low | (See DTC B1881, B1882, B1883, B1886.)
B1916 | 19 |  | Driver-side air bag module (inflator No.1) system circuit short to power supply | (See DTC B1916, B1932, B1934, B1936.)
B1925 | 21 |  | Passenger-side air bag module (inflator No.1) system circuit short to power supply | (See DTC B1925, B1933, B1935, B1938.)
B1932 | 19 |  | Driver-side air bag module (inflator No.1) system circuit resistance high | (See DTC B1916, B1932, B1934, B1936.)
B1933 | 21 |  | Passenger-side air bag module (inflator No.1) system circuit resistance high | (See DTC B1925, B1933, B1935, B1938.)
B1934 | 19 |  | Driver-side air bag module (inflator No.1) system circuit resistance low | (See DTC B1916, B1932, B1934, B1936.)
B1935 | 21 |  | Passenger-side air bag module (inflator No.1) system circuit resistance low | (See DTC B1925, B1933, B1935, B1938.)
B1936 | 19 |  | Driver-side air bag module (inflator No.1) system circuit short to ground | (See DTC B1916, B1932, B1934, B1936.)
B1938 | 21 |  | Passenger-side air bag module (inflator No.1) system circuit short to ground | (See DTC B1925, B1933, B1935, B1938.)
B1992 | 22 |  | Driver-side side air bag module circuit short to power supply | (See DTC B1992, B1993, B1994, B1995.)
B1993 | Driver-side side air bag module circuit short to body ground
B1994 | Driver-side side air bag module circuit resistance high
B1995 | Driver-side side air bag module circuit resistance low
B1996 | 23 |  | Passenger-side side air bag module circuit short to power supply | (See DTC B1996, B1997, B1998, B1999.)
B1997 | Passenger-side side air bag module circuit short to body ground
B1998 | Passenger-side side air bag module circuit resistance high
B1999 | Passenger-side side air bag module circuit resistance low
B2226 | 42 |  | Crash zone sensor system internal circuit abnormal | (See DTC B2226, B2227.)
B2227 | Crash zone sensor system communication error
B2228 | 19 |  | Driver-side air bag module (inflator No.2) system circuit short to ground | (See DTC B2228, B2230, B2232, B2234.)
B2229 | 21 |  | Passenger-side air bag module (inflator No.2) system circuit short to ground | (See DTC B2229, B2231, B2233, B2235.)
B2230 | 19 |  | Driver-side air bag module (inflator No.2) system circuit short to power supply | (See DTC B2228, B2230, B2232, B2234.)
B2231 | 21 |  | Passenger-side air bag module (inflator No.2) system circuit short to power supply | (See DTC B2229, B2231, B2233, B2235.)
B2232 | 19 |  | Driver-side air bag module (inflator No.2) system circuit resistance high | (See DTC B2228, B2230, B2232, B2234.)
B2233 | 21 |  | Passenger-side air bag module (inflator No.2) system circuit resistance high | (See DTC B2229, B2231, B2233, B2235.)
B2234 | 19 |  | Driver-side air bag module (inflator No.2) system circuit resistance low | (See DTC B2228, B2230, B2232, B2234.)
B2235 | 21 |  | Passenger-side air bag module (inflator No.2) system circuit resistance low | (See DTC B2229, B2231, B2233, B2235.)
B2444 | 43 |  | Driver-side side air bag sensor internal circuit malfunction | (See DTC B2444, U2017.)
B2445 | 44 |  | Passenger-side side air bag sensor internal circuit malfunction | (See DTC B2445, U2018.)
B2477 | 54 |  | Configuration error | (See DTC B2477.)
B2773 | 24 |  | Driver-side curtain air bag module circuit resistance low | (See DTC B2773, B2774, B2775, B2776.)
B2774 | Driver-side curtain air bag module circuit resistance high
B2775 | Driver-side curtain air bag module circuit short to body ground
B2776 | Driver-side curtain air bag module circuit short to power supply
B2777 | 25 |  | Passenger-side curtain air bag module circuit resistance low | (See DTC B2777, B2778, B2779, B2780.)
B2778 | Passenger-side curtain air bag module circuit resistance high
B2779 | Passenger-side curtain air bag module circuit short to body ground
B2780 | Passenger-side curtain air bag module circuit short to power supply
U2017 | 43 |  | Driver-side side air bag sensor communication error | (See DTC B2444, U2017.)
U2018 | 44 |  | Passenger-side side air bag sensor communication error | (See DTC B2445, U2018.)