#
MASTER CYLINDER CONSTRUCTION

id041100100700
• With the adoption of a mini-master cylinder, cylinder length is reduced and engine compartment space is easily preserved.
• With the adoption of a plunger-type (cups do not slide), 23.81 mm bore cylinder for the mini-master cylinder, durability has been improved.

  Note

  • Plunger type: A system where the cups are fixed on the side of the cylinder, and the piston slides through the inner perimeter of the cups.

• The master cylinder cannot be disassembled except for the reservoir. Therefore, if there is any malfunction in the interior of the master cylinder, replace the cylinder component without disassembling.