#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR REMOVAL/INSTALLATION [FN4A-EL]

id0517a1801100

  Warning

  • A hot transaxle and ATF can cause severe burns. Turn off the engine and wait until they are cool before replacing the ATF.

1. Remove the oil pan. (See CONTROL VALVE BODY REMOVAL [FN4A-EL].)

2. Remove the TFT sensor.

3. Install the TFT sensor.

4. Install the oil pan. (See CONTROL VALVE BODY INSTALLATION [FN4A-EL].)

5. Carry out the mechanical system test. (See MECHANICAL SYSTEM TEST [FN4A-EL].)