#
SYMPTOM TROUBLESHOOTING CHART

id0903d2812700

No. | TROUBLESHOOTING ITEM | DESCRIPTION | PAGE
--- | --- | --- | ---
1 | One or more on-board diagnostic functions inoperative. | • Malfunction in hazard warning light system, or door lock linkage system, driver's door key cylinder switch system. | (See NO. 1 ONE OR MORE ON-BOARD DIAGNOSTIC FUNCTIONS INOPERATIVE.)
2 | All on-board diagnostic functions inoperative. | • Malfunction in door lock timer unit power supply circuit, door switch circuit, cargo compartment light circuit or door lock timer unit ground circuit. | (See NO. 2 ALL ON-BOARD DIAGNOSTIC FUNCTIONS INOPERATIVE.)
3 | Transmitter ID code cannot be reprogrammed. | • Malfunction in transmitter battery, transmitter, door lock timer unit bracket, door lock timer unit bracket ground screw or door lock timer unit circuit. | (See NO. 3 TRANSMITTER ID CODE CANNOT BE REPROGRAMMED.)