#
JOINT SHAFT DISASSEMBLY/ASSEMBLY

id031300801400

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Joint shaft (See Joint Shaft Disassembly Note) (See Joint Shaft Assembly Note)
2 | Dust seal (LH) (See Dust Seal (LH) And Bearing Disassembly Note) (See Dust Seal (LH) Assembly Note)
3 | Bearing (See Dust Seal (LH) And Bearing Disassembly Note) (See Bearing Assembly Note)
4 | Dust seal (RH) (See Dust Seal (RH) Disassembly Note) (See Dust Seal (RH) Assembly Note)
5 | Bracket

## Joint Shaft Disassembly Note

1. Remove the joint shaft using a press.

## Dust Seal (LH) And Bearing Disassembly Note

1. Remove the dust seal (LH) and bearing using the SSTs.

2. If the bearing remains on the joint shaft, set the SST and joint shaft to the press.

## Dust Seal (RH) Disassembly Note

1. Remove the dust seal (RH) using the SSTs.

## Dust Seal (RH) Assembly Note

1. Apply grease to a new dust seal lip.

2. Install the dust seal (RH) using the SSTs.

## Bearing Assembly Note

1. Install a new bearing using the SSTs.

## Dust Seal (LH) Assembly Note

1. Apply grease to a new dust seal lip.

2. Install a new dust seal (LH) using the SSTs and steel plate.

## Joint Shaft Assembly Note

1. Press the joint shaft in using the SST and a press.