#
OIL PRESSURE INSPECTION [ZJ, ZY]

id011100800316

  Warning

  • Continuous exposure with USED engine oil has caused skin cancer in laboratory mice. Protect your skin by washing with soap and water immediately after this work.
  • Hot engines and engine oil can cause severe burns. Turn off the engine and wait until it and the engine oil have cooled.

1. Remove the oil pressure switch.

2. Screw the SST into the oil pressure switch installation hole.

3. Warm up the engine to normal operating temperature.

4. Run the engine at the specified speed, and note the gauge readings.

  • If not within the specification, inspect for the cause and repair or replace if necessary.

  Note

  • The oil pressure can vary with oil viscosity and temperature.

  Oil pressure (reference value) [oil temperature: 100°C {212°F}]
  330-380 kPa {3.36-3.87 kgf/cm2, 47.8-55.0 psi} min [3,000 rpm]

5. Stop the engine and wait until it is cool.

6. Remove the SST.

  Caution

  • Be sure there is no sealant between 1.0-2.0 mm {0.04-0.07 in} from the end of the oil pressure switch to prevent a possible operation malfunction.

7. Apply silicone sealant to the oil pressure switch threads.

8. Install the oil pressure switch.

  Tightening torque
  12-17 N·m {1.2-1.8 kgf·m, 9-13 ft·lbf}

9. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.