#
CLUTCH DISC INSPECTION

id051000800900

1. Using vernier calipers, measure the thickness of the lining at a rivet head on both sides.

  • If it is less than the minimum specification, replace the clutch disc.

Clutch disc minimum thickness

  0.3 mm {0.012 in}

2. Measure the clutch disc runout using a dial indicator.

  • If it exceeds the maximum specification, replace the clutch disc.

Clutch disc maximum runout

  0.7 mm {0.028 in}