#
DTC 00: ER04

id0902f6817000

DTC 00: Er04 | Cassette tape
DETECTION CONDITION | Note • When error occurs, error message "CHECK TAPE" is displayed in the LCD. • Cassette tape is worn out.
POSSIBLE CAUSE | • Tape wear • Cassette deck malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT CASSETTE TAPE • Inspect condition of cassette tape where error has occurred. • Is cassette tape okay? | Yes | Go to the next step.
No | Replace cassette tape, then go to the next step.
2 | INSPECT CASSETTE DECK • Clear DTC. • Insert cassette tape with no defect. • Play cassette tape for 20 s or more. • Start on-board diagnostic test mode. • Is DTC 00: Er04 displayed? | Yes | Replace cassette deck.
No | Troubleshooting completed.