#
NO.21 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN D, S, L RANGES, OR IN R POSITION [FN4A-EL]

id0503a1815100

21 | Noise occurs at idle when vehicle is stopped in D, S, L ranges, or in R position
DESCRIPTION | • Transaxle noisy in driving ranges when vehicle idling.
POSSIBLE CAUSE | • Although the malfunction is basically the same as No.20 "NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN ALL POSITIONS/RANGES", other causes may be selector lever position disparity or TR switch position disparity.