#
FRONT SEAT REMOVAL/INSTALLATION

id091300424400

## With Side Air Bag

  Warning

  • Handling the front seat (side air bag) improperly can accidentally deploy the side air bag, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before handling the front seat. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

1. Turn the ignition switch to the LOCK position.

2. Disconnect the negative battery cable and wait for more than 1 minute.

3. Remove in the order indicated in the table.

1 | Connector
2 | Cover
3 | Front seat

4. Install in the reverse order of removal.

## Without Side Air Bag

1. Remove in the order indicated in the table.

1 | Connector
2 | Cover
3 | Front seat

2. Install in the reverse order of removal.