#
MEMORY CLEARING PROCEDURE

id0902f6803900

1. Start the on-board diagnostic test mode.

2. First press the POWER button, then simultaneously press the AUDIO CONT button for 2 s or more.

  Caution

  • Before clearing the DTCs, be sure to enter all of them displayed in the on-board diagnostic test mode in the Audio Repair Order Form.

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.