#
COIL REMOVAL/INSTALLATION

id091400812700

  Note

  • Do not remove the coil unless you are replacing it.
  • When only the coil is replaced, the immobilizer system reprogram procedure is not necessary.

1. Disconnect the negative battery cable.

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Coil (See Coil Installation Note)

4. Install in the reverse order of removal.

## Coil Installation Note

1. Install the hole of coil to the tab of steering lock.

2. Install the hook of coil to the steering lock.