#
SHROUD PANEL REMOVAL/INSTALLATION

id091000406300

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove the front bumper reinforcement.

5. Remove the bonnet lock. (See BONNET REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

1 | Radiator mount cap
2 | Radiator mount rubber
3 | Bolt
4 | Shroud panel

7. Install in the reverse order of removal.