#
DRIVE BELT INSPECTION [ZJ, ZY]

id0110008015b7

  Note

  • Drive belt deflection/tension inspection is not necessary because of the use of the drive belt auto tensioner.

1. Remove the splash shield (RH).

2. Verify that the drive belt auto tensioner indicator mark does not exceed the limit.

  • If it exceeds the limit, replace the drive belt. (See DRIVE BELT REPLACEMENT [ZJ, ZY].)

3. Install the splash shield (RH).

Tightening torque

  7.8-10.7 N·m {80-109 kgf·cm, 69.1-94.7 in·lbf}