#
DTC TABLE [AUDIO SYSTEM]

id0902f68370d8

Screen display | Malfunction location | Page
--- | --- | ---
DTC | Output signal
09: Er22 | - | Base unit (peripheral circuit) | (See DTC 09: ER22.)
09: Er20 | - | Power supply circuit of base unit | (See DTC 09: ER20.)
00: Er10 | - | Cassette deck-base unit communication line | (See DTC 00: ER10.)
03: Er10 | - | CD player-base unit communication line | (See DTC 03: ER10.)
06: Er10 | - | CD changer (upper module)-base unit communication line | (See DTC 06: ER10.)
07: Er10 | - | MD player-base unit communication line | (See DTC 07: ER10.)
03: Er01 | - | CD player | (See DTC 03: ER01.)
03: Er02 | CHECK CD | CD player | (See DTC 03: ER02.)
03: Er07 | CHECK CD | CD player | (See DTC 03: ER07.)
00: Er01 | - | Cassette deck | (See DTC 00: ER01.)
00: Er03 | - | Cassette deck | (See DTC 00: ER03.)
00: Er04 | CHECK TAPE | Cassette tape | (See DTC 00: ER04.)
06: Er01 | - | CD changer (upper module) | (See DTC 06: ER01.)
06: Er02 | CHECK CD | CD changer (upper module) | (See DTC 06: ER02.)
06: Er07 | CHECK CD | CD changer (upper module) | (See DTC 06: ER07.)
07: Er01 | - | MD player | (See DTC 07: ER01.)
07: Er02 | CHECK MD | MD player | (See DTC 07: ER02.)
07: Er07 | CHECK MD | MD player | (See DTC 07: ER07.)
07: Er08 | - | MD | (See DTC 07: ER08.)
10: Er01, 02: Er01 | - | MP3 applicable CD player | (See DTC 10: ER01, 02: ER01.)
10: Er02, 02: Er02 | CHECK CD | MP3 applicable CD player | (See DTC 10: ER02, 02: ER02.)
10: Er07, 02: Er07 | CHECK CD | MP3 applicable CD player | (See DTC 10: ER07, 02: ER07.)
no Err | - | No stored DTCs | -