#
BAND SERVO DISASSEMBLY/ASSEMBLY

id051700116200

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Servo retainer
2 | O-ring
3 | Servo piston
4 | Servo return spring
5 | Band strut
6 | 2-4 brake band

## Assembly Procedure

1. Measure the spring free length.

Specification

Outer diameter mm {in} | Free length mm {in} | No. of coils | Wire diameter mm {in}
--- | --- | --- | ---
34.0 {1.340} | 36.4 {1.430} | 2.5 | 4.0 {0.160}

  • If not as specified, replace the spring.

2. Install the servo return spring to the transaxle case.

3. Install the servo piston to the transaxle case.

4. Apply ATF to new O-ring and install it to the transaxle case.

  O-ring inner diameter
  70.2 mm {2.76 in}

5. Install the servo retainer by tightening the bolts evenly and gradually.

Tightening torque

  10.8-13.7 N·m

  {110-140 kgf·cm, 95.5-121 in·lbf}