#
INTERIOR LIGHT REMOVAL/INSTALLATION

id091800466100

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Interior light (See Interior Light Removal Note)
2 | Connector
3 | Lens (See Lens Removal Note)
4 | Interior light bulb

3. Install in the reverse order of removal.

## Interior Light Removal Note

1. Insert a tape-wrapped flathead screwdriver into the gap between the headliner and the interior light.

2. Push the tabs, then remove the interior light.

## Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole and push it in the direction indicated by the arrow, then remove the lens.