#
PID/DATA MONITOR TABLE [MULTIPLEX COMMUNICATION SYSTEM]

id0902e6862100

PID name (definition) | WDS display | Detection state | PID monitor module | Terminal
--- | --- | --- | --- | ---
ABS_MSG (Signal reception error from the ABS HU/CU) | Present | Circuit between the ABS HU/CU and monitor module is normal. | Instrument cluster | 2W, 2X
Not Present | Circuit between the ABS HU/CU and monitor module is abnormal.
PCM_MSG (Signal reception error from PCM) | Present | Circuit between the PCM and monitor module is normal.
Not Present | Circuit between the PCM and monitor module is abnormal.