#
FLYWHEEL INSPECTION

id051000800100

1. Inspect the contact surface for scoring, cracks, and burning.

2. Remove minor scoring or burning using emery paper.

  • Repair if scoring or burning is major.
  • Replace if cracked.

3. Inspect the ring gear teeth for wear and damage.

  • If there is any malfunction, replace the flywheel.

4. Install a dial indicator on the cylinder block.

5. Measure the flywheel runout using a dial indicator.

  • If it exceeds the maximum specification, replace the flywheel.

Flywheel maximum runout

  0.13 mm {0.0051 in}