#
CURTAIN AIR BAG MODULE REMOVAL/INSTALLATION

id081000800900

  Warning

  • Handling the air bag module improperly can accidentally operate (deploy) the air bag module, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

1. Turn the ignition switch to the LOCK position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove the headliner.

4. Remove in the order indicated in the table.

1 | Connector (See Connector Removal Note.)
2 | Bolt
3 | Curtain air bag module

5. Install in the reverse order of removal.

6. Verify that the air bag system warning light illuminates for approx. 3 s and goes out when the ignition switch is turned to the ON position.

  • If the air bag system warning light does not operate, refer to the on-board diagnostic system (SRS air bag system) and perform inspection of the system.

## Connector Removal Note

1. Using a flathead screwdriver, pry out the connector stopper plate.

2. Disconnect the connector.