#
SECONDARY SHAFT COMPONENTS INSPECTION

B3E051517301103

## Gears Inspection

1. Inspect the synchronizer cones for wear.

  • If there is any malfunction, replace parts as necessary.

2. Inspect the gear teeth for damage, wear, and cracks.

  • If there is any malfunction, replace parts as necessary.

3. Inspect the synchronizer ring matching teeth for damage and wear.

  • If there is any malfunction, replace the synchronizer ring.

## Synchronizer Ring Inspection

1. Inspect the synchronizer ring teeth for damage, wear, and cracks.

  • If there is any malfunction, replace parts as necessary.

2. Inspect the tapered surface for wear and cracks.

  • If there is any malfunction, replace parts as necessary.

3. Measure the clearance between the synchronizer ring and the side of gear circumferentially using a feeler gauge.

  • If it is less than the minimum specification, replace the synchronizer ring.

  Standard clearance
  1.30-1.70 mm {0.052-0.066 in}
  Minimum clearance
  1.00 mm {0.039 in}

## Clutch Hub Component Inspection

1. Inspect the clutch hub sleeve and hub operation.

  • If there is any malfunction, replace parts as necessary.

2. Inspect the gear teeth for damage, wear, and cracks.

  • If there is any malfunction, replace parts as necessary.

3. Inspect the synchronizer keys for damage, wear, and cracks.

  • If there is any malfunction, replace parts as necessary.

4. Measure the clearance between the hub sleeve and shift fork.

  • If it exceeds the maximum specification, replace the hub sleeve and shift fork as a set.

  Standard clearance
  0.10-0.36 mm {0.004-0.014 in}
  Maximum clearance
  0.86 mm {0.034 in}

## Secondary Shaft Gear Inspection

1. Inspect the gear contact surface for damage and wear.

  • If there is any malfunction, replace the secondary shaft.

2. Inspect the splines for damage and wear.

  • If there is any malfunction, replace the secondary shaft.

3. Inspect the gear teeth for damage, wear, and cracks.

  • If there is any malfunction, replace the secondary shaft.

4. Inspect the oil passage for clogging.

  • If there is any malfunction, replace the secondary shaft.

5. Measure the shaft gear runout.

  • If it exceeds the maximum specification, replace the secondary shaft.

  Maximum runout
  0.015 mm {0.0006 in}

6. Measure the clearance between the shaft gears and the gears.

  • If not within the specification, replace parts as necessary.
mm {in}

Gear | Shaft (outer dia.) | Gear (inner dia.) | Clearance
--- | --- | --- | ---
1st | 39.45-39.47 {1.553-1.554} | 39.50-39.52 {1.555-1.556} | 0.03-0.07 {0.002-0.003}
2nd | 35.15-35.17 {1.384-1.385} | 35.20-35.22 {1.386-1.387}