#
HVAC SPECIFICATIONS

id070000100300

Item | Specification
--- | ---
Heating capacity | (kW {kcal/h}) | 3.750 {3,225}
Airflow volume (during heater operation) | Blower motor | (m3/h) | 275
Electricity consumption (during heater operation) | Blower motor | (W) | 208
Cooling capacity | (kW {kcal/h}) | 4.480 {3,853}
Airflow volume (during air conditioner operation) | Blower motor | (m3/h) | 400
Electricity consumption (during air conditioner operation) | Blower motor | (W) | 267
Magnetic clutch | (W) | 46
Fan type | Blower motor | Sirocco fan
Refrigerant | Type | R-134a
Regular amount (approximate quantity) | 470 {16.6}
(g {oz})
A/C compressor | Type | Vane-rotary
Discharge capacity | 94.5 {94.5, 3.34}
(ml {cc, fl oz})
Max. allowable speed | 6,400
(rpm)
Lube oil | Type | ATMOS GU10
Sealed volume (approximate quantity) | 120 {120, 4.06}
(ml {cc, fl oz})
Magnetic clutch clearance | 0.3-0.5 {0.012-0.019}
(mm {in})
Condenser | Type | Multiflow (sub-cooling type)
Radiated heat | (kW {kcal/h}) | 4.850 {4,171}
Receiver/drier capacity | (ml {cc, fl oz}) | 180 {180, 6.35}
Desiccant | Synthetic zeolite
Expansion valve | Type | Block type
Evaporator | Type | Double-tank drawn cup
Refrigerant pressure switch | Type | Triple-pressure
Operating pressure |
(MPa {kgf/cm2, psi})
Thermal protector | Type | Bimetallic (Indirect sensing type)
Operating temperature |
(°C {°F})
Temperature control | Reheat full air mix type
Fusible plug | Melting point | (°C {°F}) | 100-107 {212-224}