#
OBD ON-BOARD SYSTEM READINESS TEST

id010200816000
• This shows OBD system operating status. If any monitor function is incomplete, the WDS or equivalent will identify which monitor function has not been completed. Fuel System and Comprehensive Components (CCM) are continuous monitoring-type functions. The oxygen sensor will be monitored under drive cycles. The OBD diagnostic system is initialized by performing the DTC cancellation procedure or disconnecting the negative battery cable.