#
FRONT SHOCK ABSORBER INSPECTION

id021300124700

1. Remove the front shock absorber from the vehicle.

2. Inspect for damage and oil leakage.

3. Inspect the rubber bushing for deterioration and wear.

4. Compress and extend the shock piston at least three times. Verify that the operational force does not change and that there is no unusual noise.

  • If not as specified, replace the shock absorber.
  (1) Compress the shock absorber piston and release it.
  (2) Verify that the piston extends fully at a normal speed.