#
REAR SIDE FRAME (PARTIAL CUTTING) INSTALLATION

id098008608200

  Caution

  • The cut-and-joint area indicates the maximum size range of the installation position.

1. Cut the new and old parts at the cut-and-join location, and bevel the parts.

2. When installing new parts, position each part so that the section measurement aligns to the standard dimensions.

3. After trial-fitting new parts, make sure the related parts fit properly.