#
DRIVE PLATE REMOVAL/INSTALLATION [FN4A-EL]

id0517a1802500

1. Remove the transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [FN4A-EL].)

2. Remove in the order indicated in the figure.

3. Install in the reverse order of removal.

1 | Drive plate mounting bolts (See Drive Plate Mounting Bolts Removal Note.)
2 | Adapter
3 | Drive plate (See Drive Plate Installation Note.)

## Drive Plate Mounting Bolts Removal Note

1. Set the SST or equivalent against the drive plate.

2. Remove the bolts and the drive plate.

## Drive Plate Installation Note

1. Remove the sealant from the bolts hole in the crankshaft and from the drive plate mounting bolts.

2. Install the drive plate.

3. Install the adapter.

4. Install the new drive plate mounting bolts.

5. Set the SST or equivalent against the drive plate.

6. Tighten the new drive plate mounting bolts in two or three steps in the order shown.

Tightening torque

  96.1-103 N·m
  {9.8-10.5 kgf·m, 70.9-75.9 ft·lbf}

7. Install the transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [FN4A-EL].)