#
DTC 00: ER01

id0902f6816800

DTC 00: Er01 | Cassette deck
DETECTION CONDITION | • Cassette deck cannot implement insert and eject commands.
POSSIBLE CAUSE | • Defective cassette tape (deformation, broken, or foreign material stuck/attached) • Cassette deck malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | • Is cassette tape able to be ejected? | Yes | Go to the next step.
No | Replace cassette deck.
2 | INSPECT CASSETTE TAPE • Inspect condition of cassette tape where error has occurred. • Is cassette tape okay? | Yes | Go to the next step.
No | Repair (remove foreign material) or replace cassette tape, then go to the next step.
3 | INSPECT CASSETTE DECK • Clear DTC. • Insert and eject cassette tape with no defect. • Start on-board diagnostic test mode. • Is DTC 00: Er01 displayed? | Yes | Replace cassette deck.
No | Troubleshooting completed.