CLUTCH PEDAL INSPECTION

id051000801100

Clutch Pedal Height Inspection

1. Measure the distance from the center of the upper surface of the pedal pad to the floor.

  • If the clutch pedal height is not within the specification, replace the clutch pedal. (See CLUTCH PEDAL REMOVAL/INSTALLATION.)

am2zzw00004173

  Clutch pedal height (Reference value)

  303 mm {11.9 in}

Clutch Pedal Free Play Inspection

1. Depress the clutch pedal by hand until clutch resistance is felt.

  • If the clutch pedal free play is not within the specification, replace the clutch pedal. (See CLUTCH PEDAL REMOVAL/INSTALLATION.)

am2zzw00004174

  Clutch pedal free play (Reference value)

  15 mm {0.59 in} or less

Clutch Pedal Disengagement Point Inspection

1. Apply the parking brake and fix the front and rear of the wheels with the wheel chocks.

2. Start the engine at idle.

3. Without depressing the clutch pedal, move the

shift lever slowly to the reverse position.

4. Hold the lever when the gear noise is heard.

5. Depress the clutch pedal slowly.

6. Hold the pedal when the gear noise stops (clutch pedal disengagement point).

7. Measure distance A, verify that they are within specification.

am2zzw00004175

  Clutch pedal disengagement stroke

  80—100 mm {3.2—3.9 in}

Clutch Switch Inspection

1. Disconnect the negative battery cable.

2. Disconnect the clutch switch connector.

3. Verify continuity as indicated in the table.

am2zzw00004176

  • If there is any malfunction, replace the clutch switch. (See CLUTCH PEDAL REMOVAL/INSTALLATION.)