#
BLOWER UNIT DISASSEMBLY/ASSEMBLY

id071100800600

1. Disassemble in the order indicated in the table.

  Caution

  • Apply only the specified grease to the link. Otherwise abnormal noise or improper operation may result.

1 | Blower motor
2 | Air intake link
3 | Air intake crank
4 | Wire clamp
5 | Air intake door
6 | Adhesive polyurethane
7 | Blower case (1)
8 | Blower case (2)

2. Assemble in the reverse order of disassembly.