#
DTC B2229, B2231, B2233, B2235

id0802a0802200

DTC | B2229 | Passenger-side air bag module (inflator No.2) system circuit short to ground
--- | --- | ---
B2231 | Passenger-side air bag module (inflator No.2) system circuit short to power supply
B2233 | Passenger-side air bag module (inflator No.2) system circuit resistance high
B2235 | Passenger-side air bag module (inflator No.2) system circuit resistance low
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • Abnormal resistance (other than 1.9-2.6 ohms) detected in the passenger-side air bag module circuit • Malfunction in the wiring harness between the passenger-side air bag module (inflator No.2) and SAS control module
POSSIBLE CAUSE | • Open or short circuit in the wiring harness between the passenger-side air bag module (inflator No.2) and SAS control module • Passenger-side air bag module (inflator No.2) malfunction • SAS control module malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT PASSENGER-SIDE AIR BAG MODULE (INFLATOR NO.2) CONNECTOR Warning • Handling the air bag system components improperly can accidentally deploy the air bag modules and pre-tensioner seat belts, which may seriously injure you. Read the service warnings before handling the air bag system components. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.) • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Remove the passenger-side air bag module. (See PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.) • Is there cracking or chipping in the passenger-side air bag module connector? | Yes | Replace the air bag wiring harness.
No | Go to the next step.
2 | VERIFY WHETHER MALFUNCTION IS IN PASSENGER-SIDE AIR BAG MODULE (INFLATOR NO.2) OR RELATED WIRING HARNESS • Connect the leads of the SST (Fuel and thermometer checker) or apply 2-ohm resistance to passenger-side air bag module (inflator No.1) connector terminals 1A and 1B, and passenger-side air bag module (inflator No.2) connector terminals 2A and 2B. • Set resistance of the SST (Fuel and thermometer checker) to the 2-ohm position. • Connect the negative battery cable. • Turn the ignition switch to the ON position. • Using the WDS or equivalent, check the following PID/DATA monitor: (See PID/DATA MONITOR TABLE.) - OD_PAB2_ST • Is the related wiring harness normal? | Yes | Replace the passenger-side air bag module. (See PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)
No | Replace the air bag wiring harness, then go to the next step.
3 | INSPECT SAS CONTROL MODULE • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Connect the passenger-side air bag module connector. • Are any one or all of the following DTCs displayed? - B2229 - B2231 - B2233 - B2235 | Yes | [Present malfunction diagnosis] Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.) [Past malfunction diagnosis] Troubleshooting completed.
No | Troubleshooting completed.