#
NEUTRAL SWITCH INSPECTION

id014000800800

  Note

  • Perform the following inspection according to the DATA MONITOR function (indicated by monitor item from here onwards).

## Continuity Inspection

1. Disconnect the negative battery cable.

2. Remove the neutral switch.

3. Verify that the continuity between terminals A and B is as indicated in the table.

  • If there is any malfunction, replace the neutral switch.
  • If the monitor item condition/specification (reference) is not within the specification, even though there is no malfunction, carry out the "Circuit Open/Short Inspection".

## Circuit Open/Short Inspection

1. Inspect the following wiring harnesses for an open or short circuit. (Continuity check)

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the wiring harness.
  - Neutral switch terminal A and PCM terminal 1AB
  - Neutral switch terminal B and body GND

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the wiring harness.
  - Neutral switch terminal A and body GND
  - Neutral switch terminal B and power supply