#
REAR BRAKE (DRUM) INSPECTION

id041100810000

## Brake Lining Thickness Inspection

1. Remove the hub spindle and drum component as a single unit.(See REAR BRAKE (DRUM) REMOVAL/INSTALLATION.)

2. Measure the thickness of the brake lining.

  • If the thickness is less than the specification, replace the brake shoe with a new one.

Minimum rear brake lining thickness

  1.0 mm {0.04 in}

## Brake Drum Inspection

1. Remove the drum component.(See REAR BRAKE (DRUM) REMOVAL/INSTALLATION.)

2. Measure the inner diameter of the brake drum.

  • If it exceeds the specification, replace the brake drum.

Maximum rear brake drum inner diameter

  204.3 mm {8.043 in}

3. Apply chalk to the inside of the drum, and rub against the drum shoe. Inspect for scratches, and uneven or abnormal wear inside the drum.

  • If there is marked partial wear of the brake drum, repair it within the maximum brake drum inner diameter or replace it.

4. After inspection, wipe the chalk off.