#
NO.25 A/C IS NOT CUT OFF UNDER WIDE OPEN THROTTLE CONDITIONS [WITHOUT WU-TWC]

id0103008031c6

25 | A/C IS NOT CUT OFF UNDER WOT CONDITIONS.
--- | ---
DESCRIPTION | The A/C compressor magnetic clutch does not disengage under WOT the conditions.
POSSIBLE CAUSE | • TP sensor malfunction • TP sensor misadjustment • Loosely installed TP sensor.

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Does the A/C compressor disengage when the A/C switch is turned off? | Yes | Go to the next step.
No | Go to the symptom troubleshooting "No.24 A/C is always on or A/C compressor runs continuously".
2 | Connect the WDS or equivalent to the DLC-2. Retrieve any continuous memory, KOEO and KOER DTCs. (See KOEO/KOER SELF-TEST.) Are any DTCs displayed? | Yes | DTC is displayed: Go to the appropriate DTC test.
No | No DTC is displayed: Inspect the TP sensor for proper adjustment.
3 | Verify test results. • If normal, return to the diagnostic index to service any additional symptoms. • If the malfunction remains, replace or reprogram the PCM.