#
PLASTIC PARTS HEAT RESISTING TEMPERATURE

id098011740200

Part Name | Code | Material Name | Heat resisting Temperature°C{°F}
--- | --- | --- | ---
WINDSHIELD MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
COWL GRILLE | PP | POLYPROPYLENE | 100 {212}
HEAD LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PP | POLYPROPYLENE | 95 {203}
RADIATOR GRILLE | PP | POLYPROPYLENE | 95 {203}
FRONT BUMPER | PP | POLYPROPYLENE | 100 {212}
FRONT FLAP | PE | POLYETHYLENE | 80 {176}
FRONT SIDE TURN LIGHT | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | PC-PBT | POLYCARBONATE-PBT | 140 {248}
OUTSIDE MIRROR | COVER | AAS | AAS | 88 {190}
BRACK | ABS | ABS | 88 {190}
COLOR | AAS | AAS | 88 {190}
REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 80 {176}
HOUSING | AES | AES | 70 {158}
REAR BUMPER | PP | POLYPROPYLENE | 100 {212}
HIGH-MOUNT BRAKE LIGHT | COVER | PP | POLYPROPYLENE | 95 {203}
LENS | PC | POLYCARBONATE | 130 {266}
ROOF MOULDING | ACS | ACS | 105 {221}
LIFTGATE GARNISH | ABS | ABS | 95 {203}
SIDE PROTECTOR | PVC | POLYVINYLCHLORIDE | 95 {203}
REAR SPOILER | PP | POLYPROPYLENE | 100 {212}
REAR FLAP | PE | POLYETHYLENE | 80 {176}
REFLECTOR | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | ABS | ABS | 70 {158}
SHROUD PANEL | PP | POLYPROPYLENE | 100 {212}

  Note

  • The application of temperatures higher then heat resisting temperatures may result in part deformation.