#
SECURITY LIGHT: DTC NOT ILLUMINATED (WDS: DTC B1342)

id0902e4632800

DTC not illuminated (B1342) | PCM is defective
--- | ---
POSSIBLE CAUSE | • Defective PCM

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
- | INSPECT PCM • Turn the ignition switch to the ON position from LOCK again. • Does WDS indicate DTC B1342 again? | Yes | Replace PCM and reprogram immobilizer system. (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.)
No | Connect connectors properly.