#
DTC C1267 [APPLIED VIN (ASSUMED): JM0 DY10Y100 100001-108401, JM6 DY10*100 100001-109000]

id0402a3168000

DTC | C1267 | ABS control
DETECTION CONDITION | • The on-board diagnostic function detects control module malfunction.
POSSIBLE CAUSE | • Malfunction of ABS HU/CM.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear DTC from memory (See Clearing DTCs Procedures) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above. • Is same DTC present? | Yes | Replace ABS CM, then go to next step.
No | Go to next step.
2 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to applicable DTC inspection.
No | Troubleshooting completed.