#
NO.24 ENGINE STALLS WHEN SHIFTED TO D, S, L RANGES, OR IN R POSITION [FN4A-EL]

id0503a1815300

24 | Engine stalls when shifted to D, S, L ranges, or in R position
DESCRIPTION | • Engine stalls when shifting from N or P position to D, S, L ranges or R position at idle.
POSSIBLE CAUSE | • The malfunction is on the engine control side (i.e. IAC system). Otherwise, the malfunction is in the input/turbine speed sensor (engine sometimes starts) or TCC circuit (engine always stalls).

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Go to symptom troubleshooting No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [WITHOUT WU-TWC].) (See NO.10 LOW IDLE/STALLS DURING DECELERATION [WITH WU-TWC].) • Is engine control system normal? | Yes | Repeat basic inspection and repair or replace any defective parts according to inspection result. (See BASIC INSPECTION [FN4A-EL].)
No | Repair or replace any defective parts according to inspection results.
2 | • Verify test results. - If normal, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Information and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace PCM.