#
CLUTCH RELEASE CYLINDER REMOVAL/INSTALLATION

id051000801300

  Caution

  • Be careful not to spill clutch fluid on a painted surface. If this should happen, wash it off immediately.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. Bleed the air. (See CLUTCH FLUID REPLACEMENT.)

4. Inspect the clutch pedal. (See CLUTCH PEDAL INSPECTION.)

1 | Clip
2 | Clutch pipe and clutch hose
3 | Clutch pipe
4 | Bracket
5 | Clutch release cylinder