#
VEHICLE SPEEDOMETER SENSOR INSPECTION (WITHOUT ABS) [F35M-R]

id0515008428a5

1. Remove the vehicle speedometer sensor.

2. Measure voltage (AC range) between terminals of the vehicle speedometer sensor while the gear is turning.

Meter needle | Action
--- | ---
Moves slightly under 5 V (AC range) | Repair wiring harness between instrument cluster and vehicle speedometer sensor.
Does not move | Replace vehicle speedometer sensor.

3. Install the vehicle speedometer sensor. (See VEHICLE SPEEDOMETER SENSOR REMOVAL/INSTALLATION (WITHOUT ABS) [F35M-R].)