#
REAR FENDER PANEL INSTALLATION

id098008745000

1. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension, then adjust the position to align it to the standard dimensions.

2. Drill holes for plug welds before installing new parts.

3. Before installing new parts, apply spot weld sealer to the wheel arch line.

4. After trial-fitting new parts, make sure the related parts fit properly.