#
FRONT FENDER PANEL REMOVAL/INSTALLATION

id091000405900

1. Disconnect the negative battery cable.

2. Remove the front side turn light.

3. Remove the windshield wiper arm and blade. (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

4. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

5. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

6. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

7. Remove the mudguard.

8. Remove the bolts, then remove the front fender panel.

9. Install in the reverse order of removal.

10. Adjust the headlight aiming. (See HEADLIGHT AIMING.)