#
WIPER AND WASHER SWITCH REMOVAL/INSTALLATION

id091900800200

1. Disconnect the negative battery cable.

2. Remove the column cover.

3. Remove in the order indicated in the table.

1 | Connector (See Connector Installation Note)
2 | Wiper and washer switch (See Wiper and Wiper Washer Installation Note)

4. Install in the reverse order of removal.

## Connector Installation Note

1. Install the wiper and washer switch harness shown in the figure onto the clock spring hook.

## Wiper and Wiper Washer Installation Note

1. Insert the wiper and washer switch groove and hook shown in the figure into the body.

2. Insert the wiper and washer switch tab into the body until it is engaged with the body.