#
AUDIO CONTROL SWITCH INSPECTION

id092000800300

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the audio control switch connector.

4. Measure the resistance and inspect for continuity between the audio control switch terminals.

  • If there is any malfunction, replace the audio control switch.