#
B-PILLAR UPPER TRIM REMOVAL/INSTALLATION

id091700459000

1. Remove the upper anchor of the front seat belt.

2. Partially peel back the seaming welt.

3. Remove the B-pillar lower trim. (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

4. Pull the B-pillar upper trim outward, then disengage clips A.

5. Disengage the tab from the body, then remove the B-pillar upper trim.

6. Install in the reverse order of removal.