CYLINDER BLOCK DISASSEMBLY (I)

id011000500600

1. Disassemble in the order indicated in the table.

bezeze00000014

1 | Thermostat cover
2 | Thermostat
3 | Knock sensor (See Knock Sensor Disassembly Note)
4 | Oil separator
5 | Water pump
6 | Oil pump
7 | Drive plate (ATX), flywheel (MTX) (See Drive Plate (ATX), Flywheel (MTX) Disassembly Note)
8 | End plate
9 | Oil filter (See Oil Filter Disassembly Note)
10 | Oil cooler
11 | Oil filter joint (See Oil Filter Joint Disassembly Note)
12 | Oil pan (See Oil Pan Disassembly Note)
13 | Oil strainer
14 | Oil pump cover
15 | Inner rotor
16 | Outer rotor
17 | Plunger plug
18 | Plunger spring
19 | Control plunger
20 | Oil pump body

Knock Sensor Disassembly Note

1. Remove the knock sensor using the SST.

bezeze00000015

Drive Plate (ATX), Flywheel (MTX) Disassembly Note

1. Lock the drive plate (ATX) or flywheel (MTX) against rotation using the SST.

bezeze00000016

2. Remove the drive plate or flywheel installation bolts.

Oil Filter Disassembly Note

1. Remove the oil filter using the SST.

bezeze00000017

Oil Filter Joint Disassembly Note

1. Remove the oil filter joint using the following procedure:

  (1) Install two appropriate nuts (M20 x 1.5) to the oil filter joint.

  am2llw00000039

  (2) Using a wrench, apply force in the direction of the arrow shown in the figure and lock the nuts.

  am2llw00000040

  (3) Using a wrench, apply force in the loosening direction for the inside nuts and remove the oil filter joint.

Oil Pan Disassembly Note

1. Remove the oil pan using a separator tool.

bezeze00000018