#
FRONT INTERNAL GEAR ONE-WAY CLUTCH COMPONENT DISASSEMBLY/ASSEMBLY

id051700116100

1. Perform the preinspection before disassembly.

(See Front Internal Gear and One-Way Clutch Component.)

2. Disassemble in the order indicated in the table.

3. Assemble in the reverse order of disassembly.

1 | One-way clutch retainer (See One-Way Clutch Retainer Disassembly Note.)
2 | Side race
3 | One-way clutch
4 | Snap ring
5 | Front internal gear

## One-Way Clutch Retainer Disassembly Note

• Remove the one-way clutch retainer using a flathead screwdriver, etc. as shown in the figure.

## Assembly Procedure

1. Install the snap ring.

2. Install the one-way clutch to the front internal gear in the direction of the arrow (on the one-way clutch) as shown in the figure.

3. Install the side race.

4. Install the one-way clutch retainer.