#
FRONT DOOR LOCK ACTUATOR INSPECTION

id091400428700

## Door Lock Actuator

1. Apply battery positive voltage to the front door lock actuator terminals and inspect the front door lock actuator operation.

  • If not as specified, replace the front door lock actuator.

Actuator operation | Terminal
--- | ---
F (A) | E (B)
Lock | B+ | GND
Unlock | GND | B+

  () :
LH

## Door Lock-link Switch

1. Inspect for continuity between the door lock-link switch terminals.

  • If not as specified, replace the front door lock actuator.