#
PURGE SOLENOID VALVE INSPECTION

CDA011618740W02

## Airflow Inspection

1. Disconnect the negative battery cable.

2. Remove the purge solenoid valve.

3. Inspect airflow between the ports under following conditions.

  • If there is no malfunction, carry out the "Circuit Open/Short Inspection".
  • If there is any malfunction, replace the purge solenoid valve.

## Circuit Open/Short Inspection

1. Inspect the following wiring harnesses for an open or short circuit. (Continuity check)

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the wiring harness.
  - Purge solenoid valve terminal A and PCM terminal 2T
  - Purge solenoid valve terminal B and PCM terminal 2AV

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the wiring harness.
  - Purge solenoid valve terminal A and body GND
  - Purge solenoid valve terminal B and power supply