#
DTC TABLE

id010200801500

## DTC table (Without WU-TWC)

×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
P0010 | CMP actuator circuit malfunction | ON | 1 | CCM | × | (See DTC P0010.)
P0011 | CMP timing over-advanced | ON | 1 | CCM | × | (See DTC P0011.)
P0012 | CMP timing over-retarded | ON | 1 | CCM | × | (See DTC P0012.)
P0031 | HO2S heater circuit low input | ON | 2 | HO2S heater | × | (See DTC P0031.)
P0032 | HO2S heater circuit high input | ON | 2 | HO2S heater | × | (See DTC P0032.)
P0102 | MAF circuit low input | ON | 1 | CCM | × | (See DTC P0102.)
P0103 | MAF circuit high input | ON | 1 | CCM | × | (See DTC P0103.)
P0112 | IAT circuit low input | ON | 1 | CCM | × | (See DTC P0112.)
P0113 | IAT circuit high input | ON | 1 | CCM | × | (See DTC P0113.)
P0117 | ECT circuit low input | ON | 1 | CCM | × | (See DTC P0117.)
P0118 | ECT circuit high input | ON | 1 | CCM | × | (See DTC P0118.)
P0122 | TP circuit low input | ON | 1 | CCM | × | (See DTC P0122.)
P0123 | TP circuit high input | ON | 1 | CCM | × | (See DTC P0123.)
P0131 | HO2S no inversion (stuck low) | ON | 2 | CCM | × | (See DTC P0131, P0132.)
P0132 | HO2S no inversion (stuck high) | ON | 2 | CCM | × | (See DTC P0131, P0132.)
P0134 | HO2S circuit no activity detected | ON | 2 | CCM | × | (See DTC P0134.)
P0171 | Fuel trim system too lean | ON | 2 | Fuel | × | (See DTC P0171.)
P0172 | Fuel trim system too rich | ON | 2 | Fuel | × | (See DTC P0172.)
P0327 | Knock sensor circuit low input | ON | 1 | CCM | × | (See DTC P0327.)
P0328 | Knock sensor circuit high input | ON | 1 | CCM | × | (See DTC P0328.)
P0335 | CKP sensor circuit malfunction | ON | 1 | CCM | × | (See DTC P0335.)
P0340 | CMP sensor circuit malfunction | ON | 1 | CCM | × | (See DTC P0340.)
P0351 | Ignition coil No.1 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0351.)
P0352 | Ignition coil No.2 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0352.)
P0353 | Ignition coil No.3 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0353.)
P0354 | Ignition coil No.4 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0354.)
P0443 | Evaporative emission control system purge control valve circuit malfunction | ON | 2 | CCM | × | (See DTC P0443.)
P0480 | Cooling fan relay No.1 control circuit malfunction | OFF | 2 | Other | × | (See DTC P0480.)
P0481 | Cooling fan relay No.2 control circuit malfunction | OFF | 2 | Other | × | (See DTC P0481.)
P0500 | Vehicle speed sensor (VSS) circuit malfunction | ON | 2 | CCM | × | (See DTC P0500.)
P0500 | Vehicle speed sensor (VSS) circuit malfunction | (See DTC TABLE [FN4A-EL].)
P0505 | Idle control system malfunction | OFF | - | Other | - | (See DTC P0505.)
P0511 | Idle control system circuit malfunction | ON | 1 | CCM | × | (See DTC P0511.)
P0537 | Evaporator temperature sensor circuit low input | OFF | 1 | Other | × | (See DTC P0537.)
P0538 | Evaporator temperature sensor circuit high input | OFF | 1 | Other | × | (See DTC P0538.)
P0602 | PCM programming error | ON | 1 | CCM | × | (See DTC P0602.)
P0610 | Control module vehicle options error | ON | 1 | CCM | × | (See DTC P0610.)
P0660 | VIS shutter valve actuator control circuit malfunction | OFF | 2 | Other | × | (See DTC P0660.)
P0668 | PCM temperature sensor circuit low input | OFF | 1 | Other | × | (See DTC P0668.)
P0669 | PCM temperature sensor circuit high input | OFF | 1 | Other | × | (See DTC P0669.)
P0706 | Transaxle range (TR) switch circuit range/performance | (See DTC TABLE [FN4A-EL].)
P0707 | Transaxle range (TR) switch circuit low input | (See DTC TABLE [FN4A-EL].)
P0708 | Transaxle range (TR) switch circuit high input | (See DTC TABLE [FN4A-EL].)
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (Stuck) | (See DTC TABLE [FN4A-EL].)
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | (See DTC TABLE [FN4A-EL].)
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | (See DTC TABLE [FN4A-EL].)
P0715 | Input/turbine speed sensor circuit malfunction | (See DTC TABLE [FN4A-EL].)
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0741 | Torque converter clutch (TCC) (stuck OFF) | (See DTC TABLE [FN4A-EL].)
P0742 | Torque converter clutch (TCC) (stuck ON) | (See DTC TABLE [FN4A-EL].)
P0745 | Pressure control solenoid malfunction | (See DTC TABLE [FN4A-EL].)
P0751 | Shift solenoid A stuck OFF | (See DTC TABLE [FN4A-EL].)
P0752 | Shift solenoid A stuck ON | (See DTC TABLE [FN4A-EL].)
P0753 | Shift solenoid A malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0756 | Shift solenoid B stuck OFF | (See DTC TABLE [FN4A-EL].)
P0757 | Shift solenoid B stuck ON | (See DTC TABLE [FN4A-EL].)
P0758 | Shift solenoid B malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0761 | Shift solenoid C stuck OFF | (See DTC TABLE [FN4A-EL].)
P0762 | Shift solenoid C stuck ON | (See DTC TABLE [FN4A-EL].)
P0763 | Shift solenoid C malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0766 | Shift solenoid D stuck OFF | (See DTC TABLE [FN4A-EL].)
P0767 | Shift solenoid D stuck ON | (See DTC TABLE [FN4A-EL].)
P0768 | Shift solenoid D malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0771 | Shift solenoid E stuck OFF | (See DTC TABLE [FN4A-EL].)
P0772 | Shift solenoid E stuck ON | (See DTC TABLE [FN4A-EL].)
P0773 | Shift solenoid E malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P1384 | Variable valve timing control system malfunction | OFF | - | Other | - | (See DTC P1384.)
P1562 | PCM +BB voltage low | ON | 1 | CCM | × | (See DTC P1562.)
P2008 | VTCS shutter valve actuator control circuit malfunction | OFF | 2 | CCM | × | (See DTC P2008.)
P2502 | Generator terminal B circuit open | OFF | 1 | Other | - | (See DTC P2502.)
P2503 | Generator output voltage signal no electricity | OFF | 1 | Other | - | (See DTC P2503.)
P2504 | Battery overcharge | OFF | 1 | Other | - | (See DTC P2504.)
U0073 | CAN bus off | (See DTC U0073, U1900, U2516.)
U0121 | PCM cannot receive any signals from ABS HU/CM | (See DTC U0073, U1900, U2516.)
U0155 | PCM cannot receive any signals from instrument cluster | (See DTC U0073, U1900, U2516.)

## DTC table (With WU-TWC)

×: Applicable
-: Not applicable

DTC No. | Condition | MIL | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
C1277 | Steering angle sensor circuit malfunction | OFF | 1 | CCM | × | (See DTC C1277.)
P0010 | CMP actuator circuit malfunction | ON | 1 | CCM | × | (See DTC P0010.)
P0011 | CMP timing over-advanced | ON | 1 | CCM | × | (See DTC P0011.)
P0012 | CMP timing over-retarded | ON | 2 | CCM | × | (See DTC P0012.)
P0031 | HO2S heater circuit low input | ON | 2 | O2 sensor heater | × | (See DTC P0031.)
P0032 | HO2S heater circuit high input | ON | 2 | O2 sensor heater | × | (See DTC P0032.)
P0102 | MAF circuit low input | ON | 1 | CCM | × | (See DTC P0102.)
P0103 | MAF circuit high input | ON | 1 | CCM | × | (See DTC P0103.)
P0107*3 | MAP circuit low input | ON | 1 | CCM | × | (See DTC P0107.)
P0108*3 | MAP circuit high input | ON | 1 | CCM | × | (See DTC P0108.)
P0112 | IAT circuit low input | ON | 1 | CCM | × | (See DTC P0112.)
P0113 | IAT circuit high input | ON | 1 | CCM | × | (See DTC P0113.)
P0117 | ECT circuit low input | ON | 1 | CCM | × | (See DTC P0117.)
P0118 | ECT circuit high input | ON | 1 | CCM | × | (See DTC P0118.)
P0122 | TP circuit low input | ON | 1 | CCM | × | (See DTC P0122.)
P0123 | TP circuit high input | ON | 1 | CCM | × | (See DTC P0123.)
P0131 | HO2S no inversion (stuck low) | ON | 2 | CCM | × | (See DTC P0131, P0132.)
P0132 | HO2S no inversion (stuck high) | ON | 2 | CCM | × | (See DTC P0131, P0132.)
P0134 | HO2S circuit no activity detected | ON | 2 | CCM | × | (See DTC P0134.)
P0171*4 | Fuel trim system too lean | ON | 2 | Fuel | × | (See DTC P0171.)
P0172*4 | Fuel trim system too rich | ON | 2 | Fuel | × | (See DTC P0172.)
P0327 | Knock sensor circuit low input | ON | 1 | CCM | × | (See DTC P0327.)
P0328 | Knock sensor circuit high input | ON | 1 | CCM | × | (See DTC P0328.)
P0335 | CKP sensor circuit malfunction | ON | 1 | CCM | × | (See DTC P0335.)
P0340 | CMP sensor circuit malfunction | ON | 1 | CCM | × | (See DTC P0340.)
P0351 | Ignition coil No.1 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0351.)
P0352 | Ignition coil No.2 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0352.)
P0353 | Ignition coil No.3 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0353.)
P0354 | Ignition coil No.4 control circuit malfunction | ON | 2 | CCM | × | (See DTC P0354.)
P0401*3 | EGR flow insufficient detected | ON | 2 | EGR system | × | (See DTC P0401.)
P0403*3 | EGR control circuit problem | ON | 2 | CCM | × | (See DTC P0403.)
P0443 | Evaporative emission control system purge control valve circuit malfunction | ON | 2 | CCM | × | (See DTC P0443.)
P0480 | Cooling fan relay No.1 control circuit malfunction | OFF | 2 | Other | × | (See DTC P0480.)
P0481 | Cooling fan relay No.2 control circuit malfunction | OFF | 2 | Other | × | (See DTC P0481.)
P0500*1 | Vehicle speed sensor (VSS) circuit malfunction | ON | 2 | CCM | × | (See DTC P0500.)
P0500*2 | Vehicle speed sensor (VSS) circuit malfunction | (See DTC TABLE [FN4A-EL].)
P0505 | Idle control system malfunction | OFF | - | Other | - | (See DTC P0505.)
P0511 | Idle control system circuit malfunction | ON | 1 | CCM | × | (See DTC P0511.)
P0537 | Evaporator temperature sensor circuit low input | OFF | 1 | Other | × | (See DTC P0537.)
P0538 | Evaporator temperature sensor circuit high input | OFF | 1 | Other | × | (See DTC P0538.)
P0602 | PCM programming error | ON | 1 | CCM | × | (See DTC P0602.)
P0610 | Control module vehicle options error | ON | 1 | CCM | × | (See DTC P0610.)
P0660 | VIS shutter valve actuator control circuit malfunction | OFF | 2 | Other | × | (See DTC P0660.)
P0668 | PCM temperature sensor circuit low input | OFF | 1 | Other | × | (See DTC P0668.)
P0669 | PCM temperature sensor circuit high input | OFF | 1 | Other | × | (See DTC P0669.)
P0706*2 | Transaxle range (TR) switch circuit range/performance | (See DTC TABLE [FN4A-EL].)
P0707*2 | Transaxle range (TR) switch circuit low input | (See DTC TABLE [FN4A-EL].)
P0708*2 | Transaxle range (TR) switch circuit high input | (See DTC TABLE [FN4A-EL].)
P0711*2 | Transaxle fluid temperature (TFT) sensor circuit range/performance (Stuck) | (See DTC TABLE [FN4A-EL].)
P0712*2 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | (See DTC TABLE [FN4A-EL].)
P0713*2 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | (See DTC TABLE [FN4A-EL].)
P0715*2 | Input/turbine speed sensor circuit malfunction | (See DTC TABLE [FN4A-EL].)
P0731*2 | Gear 1 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0732*2 | Gear 2 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0733*2 | Gear 3 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0734*2 | Gear 4 incorrect (incorrect gear ratio detected) | (See DTC TABLE [FN4A-EL].)
P0741*2 | Torque converter clutch (TCC) (stuck OFF) | (See DTC TABLE [FN4A-EL].)
P0742*2 | Torque converter clutch (TCC) (stuck ON) | (See DTC TABLE [FN4A-EL].)
P0745*2 | Pressure control solenoid malfunction | (See DTC TABLE [FN4A-EL].)
P0751*2 | Shift solenoid A stuck OFF | (See DTC TABLE [FN4A-EL].)
P0752*2 | Shift solenoid A stuck ON | (See DTC TABLE [FN4A-EL].)
P0753*2 | Shift solenoid A malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0756*2 | Shift solenoid B stuck OFF | (See DTC TABLE [FN4A-EL].)
P0757*2 | Shift solenoid B stuck ON | (See DTC TABLE [FN4A-EL].)
P0758*2 | Shift solenoid B malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0761*2 | Shift solenoid C stuck OFF | (See DTC TABLE [FN4A-EL].)
P0762*2 | Shift solenoid C stuck ON | (See DTC TABLE [FN4A-EL].)
P0763*2 | Shift solenoid C malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0766*2 | Shift solenoid D stuck OFF | (See DTC TABLE [FN4A-EL].)
P0767*2 | Shift solenoid D stuck ON | (See DTC TABLE [FN4A-EL].)
P0768*2 | Shift solenoid D malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0771*2 | Shift solenoid E stuck OFF | (See DTC TABLE [FN4A-EL].)
P0772*2 | Shift solenoid E stuck ON | (See DTC TABLE [FN4A-EL].)
P0773*2 | Shift solenoid E malfunction (electrical) | (See DTC TABLE [FN4A-EL].)
P0894*2 | Forward clutch torque transmission | (See DTC TABLE [FN4A-EL].)
P1384 | Variable valve timing control system malfunction | OFF | - | Other | - | (See DTC P1384.)
P1562 | PCM +BB voltage low | ON | 1 | CCM | × | (See DTC P1562.)
P2008 | VTCS shutter valve actuator control circuit malfunction | ON | 2 | CCM | × | (See DTC P2008.)
P2177*3 | System too lean off idle | ON | 2 | Fuel | × | (See DTC P2177.)
P2178*3 | System too rich off idle | ON | 2 | Fuel | × | (See DTC P2178.)
P2187*3 | System too lean at idle | ON | 2 | Fuel | × | (See DTC P2187.)
P2188*3 | System too rich at idle | ON | 2 | Fuel | × | (See DTC P2188.)
P2502 | Generator terminal B circuit open | OFF | 1 | Other | × | (See DTC P2502.)
P2503 | Generator output voltage signal no electricity | OFF | 1 | Other | × | (See DTC P2503.)
P2504 | Battery overcharge | OFF | 1 | Other | × | (See DTC P2504.)
U0073 | CAN bus off | (See DTC U0073, U1900, U2516.)
U0121 | PCM cannot receive any signals from ABS HU/CM | (See DTC U0073, U1900, U2516.)
U0155 | PCM cannot receive any signals from instrument cluster | (See DTC U0073, U1900, U2516.)

  *1 :
MTX
  *2 :
ATX
  *3 :
With EGR system
  *4 :
Without EGR system