#
FUEL FILTER (HIGH-PRESSURE) REMOVAL/INSTALLATION

id011400803000

1. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE.)

2. Disconnect the negative battery cable.

3. Lift up the vehicle.

4. Remove in the order indicated in the table.

1 | Quick release connector (See FUEL HOSE (FUEL TANK SIDE) REMOVAL/INSTALLATION)
2 | Quick release connector (See Quick Release Connector Removal Note) (See FUEL HOSE (FUEL TANK SIDE) REMOVAL/INSTALLATION)
3 | Fuel filter (high-pressure)

5. Install in the reverse order of removal.

6. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.)

## Quick Release Connector Removal Note

1. The quick release connector can be disconnected easily after the fuel filter (high-pressure) is removed from the bracket.